BANSHEE TEAM 
                    README

             <<<Banshee Evolution 0.9>>>

SEPTEMBER 2003- 

>>Voodoo Banshee Windows(r) 9x AGP/PCI Driver Kit<<

Win9x 2D/3D Display Drivers: 4.12.01.1222  
Voodoo Banshee Glide(tm) 2.X Driver:  2.61.00.0674 
Voodoo Banshee Glide 3.X Driver: 3.10.00.30303 http://glide.sourceforge.net/
Voodoo Banshee Control Panel: 4.12.01.1552
OpenGL ICD Interceptor:   1.00.01.0106 http://www.users.on.net/triforce/glidexp/
OpenGL(r) Driver Version: 1.0.0.0761 ICD

Fresh Installation- 

1) Extract the files for the Voodoo Banshee driver to a directory.
2) Before removing your existing 2D card switch the video driver to 
   Standard VGA. Click Start, Control Panel. Double-click on Display.

   Select 640X480 and 16 colors.  Accept the changes.

3) Power off the system and remove your existing 2D card.
4) Install the Voodoo Banshee Card in a free AGP/PCI Slot
5) Power on the system and verify that video appears during post.
6) Start Windows in Normal mode

  (Once Windows starts you may be notified that no video device
   exists, click Cancel if this message appears)

7) Windows will detect a new VGA Compatible Display. You need to:

                            Windows 98: Click the Next Button on the Detection 
                                        Dialog Box and in the "Specify a 
                                        Location" field click the checkbox 
                                        then enter the path to the Win98
                                        directory in the drivers location.

8) You may then be prompted to insert the Banshee Evolution Source Disk.  
   Again, enter the path you specified in Step 1 and press OK.
9) Windows will copy the drivers. Reboot the system when prompted
10) Install DirectX 9.0.

Upgrade Existing Voodoo Banshee Drivers-

1) Start Windows 98
2) Extract the files for the Voodoo Banshee driver to a directory.
3) Click Start, Control Panel.  Double-click on Display.
4) Click the Settings tab then click:

                      Windows 98 users: Click "Advanced Properties"

5) Then under "Change Display Type/Advanced Display" click "Change"
6) Click "Have Disk" and enter the path specified in Step 2 plus:

                      Windows 98 users: the Win98 directory.

7) When asked to choose a device, select "3dfx Voodoo Banshee"
8) You may then be prompted to insert the Banshee Evolution Source Disk.
   Enter the path you specified in Step 2 again.
9) Windows will copy the drivers.   Reboot the system when prompted.
10) Install DirectX 9.0

Know Limitations-

No multitexturing yet, some games like Medal of Honor will not start. 
No T&L support, some recent games will not start. For Unreal Tournament 2003 use ufficial patch, for Tennis Master Series 2003 use 3DAnalyse.
Neverwinter Nights will start with software rendering but very slow.
Fixed in this driver-
Fixed errors in QuakeIII arena based games(Bid For Power now run very well).
Jedi Knight 2 and Star Trek Voyager Elite Force now should run without problem.

What's new?-

Added 60Hz, 75Hz, and 85Hz on smaller (14") fix for Voodoo Banshee users.
New Glide core.
New optimization.